November 7. 2013 inspection comments continued

After reviewing the records we inspected the emission units.

There was no coal or equipment for handling coal in the fuel yard (EU008); according to the 2012 and 2011 AORs no coal has been received in 2011 or 2012. According to the March 12, 2012 FCE inspection the facility has not received any coal since 2003.

Each gas turbine system emissions unit was equipped with a Continuous Emission Monitoring System (CEMS) in the exhaust stack as required by Specific Condition No. A.14. See the Emission unit section for model and serial number of CEM equipment. I noted pipes for the water injection systems at the gas turbines.

I left the facility at approximately 2:30 pm.

Pictures are located on the EPC I drive at:

I:\NOEL\Compliance folder\TECO\0570040\2014 FCE